1m sec
------

V(vin)*((I(L1)+I(L2)+I(L3)+I(L4))*2) = 76.044mJ integral = 76.044KW average

V(vin)/((I(L1)+I(L2)+I(L3)+I(L4))*2) = 1.4822ohm average

[Coil Voltage] V(vin) = 346.1V RMS

[Coil Amperage] (I(L1)+I(L2)+I(L3)+I(L4))*2 = 219.73A RMS

[DEAD BATTERY = oNE Femto Volt] I(v) = 138.44mA RMS [pos/neg charging with A/C]